February 27, 2019

These items are not accepted in **SCRAP METAL LOADS**:

Acetylene Cylinders

Any scrap with small capacitors

Anything containing Freon – Must be extracted prior to pick up.

Asbestos Containing Material

Asphalt

Beer kegs

Biohazard Waste or anything with blood or human fluids

Carpet

Catalytic converters

Ceramic Tiles

Clay

Closed compress air cans

Concrete

Corrosive Material – high acid like battery acid

CRT – Cathode Ray Tubes - for example computer monitors, televisions

Debris – anything classified as debris

Dirt

Explosive Materials – Gun shells

Fiberglass

Foam

Funeral Markers, or vases

Furniture

Gas Tank(s) – Must be empty and have been cleaned. All tank(s) should be verified that are empty & clean

Hazardous waste – Toxic or poisonous

Historical Markers

Insulation

Liquids – water, and antifreeze, hydraulic fluid, paint, etc

Mercury containing material – fluorescent light bulbs

Paint cans, degreasers

Particle Board

PCB Containing material

Plastic

Propane Tanks – All sizes

Radioactive scrap

Rubber

Shopping Carts

Styrofoam

Tires

Wood